{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:01.182 Starting lwIP, IPv4 disable\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:01.183 ip6 linklocal address: FE80::200:23FF:FE48:BE18\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

Download START ALL

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:03.854 initializing aboot release package...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:03.855 extracting download.json (2 KB)...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:03.855 extracting partition.bin (2 KB)...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "commands" : [
      {
         "command" : "require",
         "group" : "0",
         "image" : null,
         "name" : "product",
         "value" : "arom-tiny"
      },
      {
         "command" : "require",
         "group" : "0",
         "image" : null,
         "name" : "version",
         "value" : "0.5"
      },
      {
         "command" : "require",
         "group" : "0",
         "image" : null,
         "name" : "version-bootrom",
         "value" : "2021.10.16"
      },
      {
         "command" : "progress",
         "group" : "0",
         "image" : null,
         "name" : "weight",
         "value" : 10313728
      },
      {
         "command" : "call",
         "group" : "0",
         "image" : "preboot.img",
         "imageSize" : 17188,
         "version-bootrom" : null
      },
      {
         "command" : "call",
         "group" : "0",
         "image" : "flasher.img",
         "imageSize" : 31592,
         "version-bootrom" : null
      },
      {
         "command" : "identify",
         "group" : "0",
         "image" : "board.id",
         "imageSize" : 21,
         "version-bootrom" : null
      },
      {
         "command" : "partition",
         "group" : "0",
         "image" : "flashinfo.bin",
         "imageSize" : 648,
         "version-bootrom" : null
      },
      {
         "command" : "partition",
         "group" : "0",
         "image" : "partition.bin",
         "imageSize" : 2188,
         "version-bootrom" : null
      },
      {
         "command" : "flash",
         "group" : "1",
         "image" : "bootloader.ubi",
         "imageSize" : 77824,
         "partition" : "bootloader",
         "version-bootrom" : null,
         "weight" : 167936
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "partition.bin",
         "imageSize" : 2188,
         "partition" : "ptable",
         "version-bootrom" : null,
         "weight" : 8192
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "fwcerts.bin",
         "imageSize" : 2036,
         "partition" : "fwcerts",
         "version-bootrom" : null,
         "weight" : 16384
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "ReliableData.bin",
         "imageSize" : 32768,
         "partition" : "rd",
         "version-bootrom" : null,
         "weight" : 65536
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "apn.bin",
         "imageSize" : 23922,
         "partition" : "apn",
         "version-bootrom" : null,
         "weight" : 57344
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "cp.bin",
         "imageSize" : 4653056,
         "partition" : "cp",
         "version-bootrom" : null,
         "weight" : 9306112
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "dsp.bin",
         "imageSize" : 65691,
         "partition" : "dsp",
         "version-bootrom" : null,
         "weight" : 139264
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "rf.bin",
         "imageSize" : 1942,
         "partition" : "rfbin",
         "version-bootrom" : null,
         "weight" : 8192
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "logo.bin",
         "imageSize" : 22628,
         "partition" : "logo",
         "version-bootrom" : null,
         "weight" : 49152
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "updater.bin",
         "imageSize" : 60620,
         "partition" : "updater",
         "version-bootrom" : null,
         "weight" : 126976
      },
      {
         "command" : "erase",
         "group" : "3",
         "image" : null,
         "partition" : "fota_param",
         "weight" : 12288
      },
      {
         "command" : "erase",
         "group" : "3",
         "image" : null,
         "partition" : "fota_pkg",
         "weight" : 4096
      },
      {
         "command" : "erase",
         "group" : "4",
         "image" : null,
         "partition" : "nvm",
         "weight" : 319488
      },
      {
         "command" : "erase",
         "group" : "5",
         "image" : null,
         "partition" : "factory",
         "productionOnly" : true,
         "weight" : 32768
      }
   ],
   "event" : 1,
   "partitions" : [
      {
         "depth" : 0,
         "name" : "all",
         "size" : 8388608,
         "start" : 0,
         "type" : "group",
         "vsize" : 8388608,
         "vstart" : -1
      },
      {
         "depth" : 1,
         "name" : "qspi",
         "size" : 8388608,
         "start" : 0,
         "type" : "flash",
         "vsize" : 8388608,
         "vstart" : 2147483648
      },
      {
         "depth" : 2,
         "name" : "bootloader",
         "size" : 90112,
         "start" : 0,
         "type" : "ubi",
         "vsize" : 90112,
         "vstart" : 2147483648
      },
      {
         "depth" : 2,
         "name" : "system",
         "size" : 4833280,
         "start" : 90112,
         "type" : "part",
         "vsize" : 4833280,
         "vstart" : 2147573760
      },
      {
         "depth" : 3,
         "name" : "ptable",
         "size" : 4096,
         "start" : 90112,
         "type" : "raw",
         "vsize" : 2188,
         "vstart" : 2147573760
      },
      {
         "depth" : 3,
         "name" : "fwcerts",
         "size" : 12288,
         "start" : 94208,
         "type" : "raw",
         "vsize" : 2036,
         "vstart" : 2147577856
      },
      {
         "depth" : 3,
         "name" : "rd",
         "size" : 32768,
         "start" : 106496,
         "type" : "raw",
         "vsize" : 32768,
         "vstart" : 2147590144
      },
      {
         "depth" : 3,
         "name" : "apn",
         "size" : 32768,
         "start" : 139264,
         "type" : "raw",
         "vsize" : 23922,
         "vstart" : 2147622912
      },
      {
         "depth" : 3,
         "name" : "cp",
         "size" : 4653056,
         "start" : 172032,
         "type" : "raw",
         "vsize" : 4653056,
         "vstart" : 2147655680
      },
      {
         "depth" : 3,
         "name" : "dsp",
         "size" : 69632,
         "start" : 4825088,
         "type" : "raw",
         "vsize" : 65691,
         "vstart" : 2152308736
      },
      {
         "depth" : 3,
         "name" : "rfbin",
         "size" : 4096,
         "start" : 4894720,
         "type" : "raw",
         "vsize" : 1942,
         "vstart" : 2152378368
      },
      {
         "depth" : 3,
         "name" : "logo",
         "size" : 24576,
         "start" : 4898816,
         "type" : "raw",
         "vsize" : 22628,
         "vstart" : 2152382464
      },
      {
         "depth" : 2,
         "name" : "reserved",
         "size" : 3031040,
         "start" : 4923392,
         "type" : "raw",
         "vsize" : 3031040,
         "vstart" : 2152407040
      },
      {
         "depth" : 2,
         "name" : "fota_param",
         "size" : 12288,
         "start" : 7954432,
         "type" : "raw",
         "vsize" : 12288,
         "vstart" : 2155438080
      },
      {
         "depth" : 2,
         "name" : "updater",
         "size" : 65536,
         "start" : 7966720,
         "type" : "raw",
         "vsize" : 60620,
         "vstart" : 2155450368
      },
      {
         "depth" : 2,
         "name" : "fota_pkg",
         "size" : 4096,
         "start" : 8032256,
         "type" : "raw",
         "vsize" : 4096,
         "vstart" : 2155515904
      },
      {
         "depth" : 2,
         "name" : "nvm",
         "size" : 319488,
         "start" : 8036352,
         "type" : "raw",
         "vsize" : 319488,
         "vstart" : 2155520000
      },
      {
         "depth" : 2,
         "name" : "factory",
         "size" : 32768,
         "start" : 8355840,
         "type" : "part",
         "vsize" : 32768,
         "vstart" : 2155839488
      },
      {
         "depth" : 3,
         "name" : "factory_a",
         "size" : 32768,
         "start" : 8355840,
         "type" : "raw",
         "vsize" : 32768,
         "vstart" : 2155839488
      }
   ]
}

### ABOOT_EVENT_DOWNLOAD_INIT ###

{
   "commands" : [
      {
         "command" : "require",
         "group" : "0",
         "image" : null,
         "name" : "product",
         "value" : "arom-tiny"
      },
      {
         "command" : "require",
         "group" : "0",
         "image" : null,
         "name" : "version",
         "value" : "0.5"
      },
      {
         "command" : "require",
         "group" : "0",
         "image" : null,
         "name" : "version-bootrom",
         "value" : "2021.10.16"
      },
      {
         "command" : "progress",
         "group" : "0",
         "image" : null,
         "name" : "weight",
         "value" : 10313728
      },
      {
         "command" : "call",
         "group" : "0",
         "image" : "preboot.img",
         "imageSize" : 17188,
         "version-bootrom" : null
      },
      {
         "command" : "call",
         "group" : "0",
         "image" : "flasher.img",
         "imageSize" : 31592,
         "version-bootrom" : null
      },
      {
         "command" : "identify",
         "group" : "0",
         "image" : "board.id",
         "imageSize" : 21,
         "version-bootrom" : null
      },
      {
         "command" : "partition",
         "group" : "0",
         "image" : "flashinfo.bin",
         "imageSize" : 648,
         "version-bootrom" : null
      },
      {
         "command" : "partition",
         "group" : "0",
         "image" : "partition.bin",
         "imageSize" : 2188,
         "version-bootrom" : null
      },
      {
         "command" : "flash",
         "group" : "1",
         "image" : "bootloader.ubi",
         "imageSize" : 77824,
         "partition" : "bootloader",
         "version-bootrom" : null,
         "weight" : 167936
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "partition.bin",
         "imageSize" : 2188,
         "partition" : "ptable",
         "version-bootrom" : null,
         "weight" : 8192
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "fwcerts.bin",
         "imageSize" : 2036,
         "partition" : "fwcerts",
         "version-bootrom" : null,
         "weight" : 16384
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "ReliableData.bin",
         "imageSize" : 32768,
         "partition" : "rd",
         "version-bootrom" : null,
         "weight" : 65536
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "apn.bin",
         "imageSize" : 23922,
         "partition" : "apn",
         "version-bootrom" : null,
         "weight" : 57344
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "cp.bin",
         "imageSize" : 4653056,
         "partition" : "cp",
         "version-bootrom" : null,
         "weight" : 9306112
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "dsp.bin",
         "imageSize" : 65691,
         "partition" : "dsp",
         "version-bootrom" : null,
         "weight" : 139264
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "rf.bin",
         "imageSize" : 1942,
         "partition" : "rfbin",
         "version-bootrom" : null,
         "weight" : 8192
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "logo.bin",
         "imageSize" : 22628,
         "partition" : "logo",
         "version-bootrom" : null,
         "weight" : 49152
      },
      {
         "command" : "flash",
         "group" : "2",
         "image" : "updater.bin",
         "imageSize" : 60620,
         "partition" : "updater",
         "version-bootrom" : null,
         "weight" : 126976
      },
      {
         "command" : "erase",
         "group" : "3",
         "image" : null,
         "partition" : "fota_param",
         "weight" : 12288
      },
      {
         "command" : "erase",
         "group" : "3",
         "image" : null,
         "partition" : "fota_pkg",
         "weight" : 4096
      },
      {
         "command" : "erase",
         "group" : "4",
         "image" : null,
         "partition" : "nvm",
         "weight" : 319488
      },
      {
         "command" : "erase",
         "group" : "5",
         "image" : null,
         "partition" : "factory",
         "productionOnly" : true,
         "weight" : 32768
      }
   ],
   "event" : 1,
   "partitions" : [
      {
         "depth" : 0,
         "name" : "all",
         "size" : 8388608,
         "start" : 0,
         "type" : "group",
         "vsize" : 8388608,
         "vstart" : -1
      },
      {
         "depth" : 1,
         "name" : "qspi",
         "size" : 8388608,
         "start" : 0,
         "type" : "flash",
         "vsize" : 8388608,
         "vstart" : 2147483648
      },
      {
         "depth" : 2,
         "name" : "bootloader",
         "size" : 90112,
         "start" : 0,
         "type" : "ubi",
         "vsize" : 90112,
         "vstart" : 2147483648
      },
      {
         "depth" : 2,
         "name" : "system",
         "size" : 4833280,
         "start" : 90112,
         "type" : "part",
         "vsize" : 4833280,
         "vstart" : 2147573760
      },
      {
         "depth" : 3,
         "name" : "ptable",
         "size" : 4096,
         "start" : 90112,
         "type" : "raw",
         "vsize" : 2188,
         "vstart" : 2147573760
      },
      {
         "depth" : 3,
         "name" : "fwcerts",
         "size" : 12288,
         "start" : 94208,
         "type" : "raw",
         "vsize" : 2036,
         "vstart" : 2147577856
      },
      {
         "depth" : 3,
         "name" : "rd",
         "size" : 32768,
         "start" : 106496,
         "type" : "raw",
         "vsize" : 32768,
         "vstart" : 2147590144
      },
      {
         "depth" : 3,
         "name" : "apn",
         "size" : 32768,
         "start" : 139264,
         "type" : "raw",
         "vsize" : 23922,
         "vstart" : 2147622912
      },
      {
         "depth" : 3,
         "name" : "cp",
         "size" : 4653056,
         "start" : 172032,
         "type" : "raw",
         "vsize" : 4653056,
         "vstart" : 2147655680
      },
      {
         "depth" : 3,
         "name" : "dsp",
         "size" : 69632,
         "start" : 4825088,
         "type" : "raw",
         "vsize" : 65691,
         "vstart" : 2152308736
      },
      {
         "depth" : 3,
         "name" : "rfbin",
         "size" : 4096,
         "start" : 4894720,
         "type" : "raw",
         "vsize" : 1942,
         "vstart" : 2152378368
      },
      {
         "depth" : 3,
         "name" : "logo",
         "size" : 24576,
         "start" : 4898816,
         "type" : "raw",
         "vsize" : 22628,
         "vstart" : 2152382464
      },
      {
         "depth" : 2,
         "name" : "reserved",
         "size" : 3031040,
         "start" : 4923392,
         "type" : "raw",
         "vsize" : 3031040,
         "vstart" : 2152407040
      },
      {
         "depth" : 2,
         "name" : "fota_param",
         "size" : 12288,
         "start" : 7954432,
         "type" : "raw",
         "vsize" : 12288,
         "vstart" : 2155438080
      },
      {
         "depth" : 2,
         "name" : "updater",
         "size" : 65536,
         "start" : 7966720,
         "type" : "raw",
         "vsize" : 60620,
         "vstart" : 2155450368
      },
      {
         "depth" : 2,
         "name" : "fota_pkg",
         "size" : 4096,
         "start" : 8032256,
         "type" : "raw",
         "vsize" : 4096,
         "vstart" : 2155515904
      },
      {
         "depth" : 2,
         "name" : "nvm",
         "size" : 319488,
         "start" : 8036352,
         "type" : "raw",
         "vsize" : 319488,
         "vstart" : 2155520000
      },
      {
         "depth" : 2,
         "name" : "factory",
         "size" : 32768,
         "start" : 8355840,
         "type" : "part",
         "vsize" : 32768,
         "vstart" : 2155839488
      },
      {
         "depth" : 3,
         "name" : "factory_a",
         "size" : 32768,
         "start" : 8355840,
         "type" : "raw",
         "vsize" : 32768,
         "vstart" : 2155839488
      }
   ]
}

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:03.857 initialized aboot release package successfully.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.005 starting aboot download engine...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.005 extracting download.json (2 KB)...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.006 download engine running in production mode!\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 2
}

### ABOOT_EVENT_DOWNLOAD_START ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.006 aboot download engine started successfully.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.006 getting serial devices list...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "description" : "Arom Usb Boot Port",
   "displayName" : "ASR Serial Download Device (COM10)",
   "enabled" : false,
   "event" : 5,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "order" : 0,
   "path" : "COM10",
   "productId" : 12292,
   "progress" : 0,
   "status" : "ONLINE",
   "triggered" : false,
   "vendorId" : 11980
}

{
   "description" : "Arom Usb Boot Port",
   "displayName" : "ASR Serial Download Device (COM16)",
   "enabled" : false,
   "event" : 5,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "order" : 0,
   "path" : "COM16",
   "productId" : 12292,
   "progress" : 0,
   "status" : "ONLINE",
   "triggered" : false,
   "vendorId" : 11980
}

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.007 <COM10> new device arrived.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.007 <COM16> new device arrived.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "description" : "Arom Usb Boot Port",
   "displayName" : "ASR Serial Download Device (COM10)",
   "enabled" : true,
   "event" : 6,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "order" : 1,
   "path" : "COM10",
   "productId" : 12292,
   "progress" : 0,
   "status" : "CONNECTING",
   "triggered" : true,
   "vendorId" : 11980
}

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.236 enabling device <COM10> into downloading mode...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.236 device <COM10> enabled successfully.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.236 connecting to serial device <COM10>...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "description" : "Arom Usb Boot Port",
   "displayName" : "ASR Serial Download Device (COM16)",
   "enabled" : true,
   "event" : 6,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "order" : 2,
   "path" : "COM16",
   "productId" : 12292,
   "progress" : 0,
   "status" : "CONNECTING",
   "triggered" : true,
   "vendorId" : 11980
}

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.252 enabling device <COM16> into downloading mode...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.252 device <COM16> enabled successfully.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "",
   "message" : "11:18:04.252 connecting to serial device <COM16>...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:04.255 <COM10> connected to serial device <COM10> successfully!\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:04.255 <COM10> starting to fire device <COM10>...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:04.256 <COM10> ONLINE device_open_failed_num = 0, device_list size = 1\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:04.256 <COM10> device <COM10> fired successfully.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:04.271 <COM16> connected to serial device <COM16> successfully!\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:04.271 <COM16> starting to fire device <COM16>...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:04.271 <COM16> ONLINE device_open_failed_num = 0, device_list size = 2\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:04.271 <COM16> device <COM16> fired successfully.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.395 <COM16> device <COM16> is ready to be enabled manually\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.396 <COM10> device <COM10> is ready to be enabled manually\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "description" : "Arom Usb Boot Port",
   "displayName" : "ASR Serial Download Device (COM16)",
   "enabled" : true,
   "event" : 6,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "order" : 2,
   "path" : "COM16",
   "productId" : 12292,
   "progress" : 0,
   "status" : "RUNNING",
   "triggered" : false,
   "vendorId" : 11980
}

{
   "description" : "Arom Usb Boot Port",
   "displayName" : "ASR Serial Download Device (COM10)",
   "enabled" : true,
   "event" : 6,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "order" : 1,
   "path" : "COM10",
   "productId" : 12292,
   "progress" : 0,
   "status" : "RUNNING",
   "triggered" : false,
   "vendorId" : 11980
}

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.489 <COM16> processing command [get bootrom info]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.490 <COM10> processing command [get bootrom info]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.496 <COM16> BOARD_ID: \n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.496 <COM16> processing command [require product arom-tiny]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.496 <COM16> Checking product\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.496 <COM10> BOARD_ID: \n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.496 <COM10> processing command [require product arom-tiny]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.496 <COM10> Checking product\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.497 <COM16> OKAY [  0.001s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.497 <COM16> processing command [require version 0.5]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.497 <COM16> Checking version\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.497 <COM10> OKAY [  0.001s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.497 <COM10> processing command [require version 0.5]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.497 <COM10> Checking version\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.497 <COM16> OKAY [  0.001s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.497 <COM16> processing command [require version-bootrom 2021.10.16]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.497 <COM16> Checking version-bootrom\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.497 <COM10> OKAY [  0.001s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.497 <COM10> processing command [require version-bootrom 2021.10.16]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.497 <COM10> Checking version-bootrom\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.498 <COM16> OKAY [  0.001s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.498 <COM16> processing command [progress weight 10313728]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.498 <COM16> setting total progress\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.498 <COM10> OKAY [  0.001s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.498 <COM10> processing command [progress weight 10313728]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.498 <COM10> setting total progress\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.499 <COM16> OKAY [  0.001s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.499 <COM10> OKAY [  0.001s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.500 <COM16> target reported max download size of 75888 bytes\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.500 <COM10> target reported max download size of 75888 bytes\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.500 <COM16> extracting preboot.img (16 KB)...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.501 <COM16> processing command [call preboot.img]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.501 <COM10> processing command [call preboot.img]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.501 <COM16> Sending 'preboot.img' (16 KB)\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.501 <COM10> Sending 'preboot.img' (16 KB)\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.537 <COM16> OKAY [  0.035s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.537 <COM16> verifying\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.537 <COM10> OKAY [  0.035s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.537 <COM10> verifying\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.623 <COM16> #=> [INFO: BlCommon  ] Loading image from #0xd1f0d818 to #0x80 with size 27520 successfully.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.623 <COM16> OKAY [  0.086s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.623 <COM16> calling\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.624 <COM10> #=> [INFO: BlCommon  ] Loading image from #0xd1f0d818 to #0x80 with size 27520 successfully.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.624 <COM10> OKAY [  0.087s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.624 <COM10> calling\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [INFO: Freq      ] Freq change done: CR5 624MHz -> 624MHz, AXI 208MHz -> 208MHz\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [PRI : Preboot   ] Executing preboot application...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [PRI : Preboot   ] Preboot version: 2022.04.12\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [INFO: EFuse     ] lotid[0..5]: 36 24 23 32 5 6\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [INFO: EFuse     ] X_location: 88, Y_location: 120, Wafer: 7\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [PRI : PMIC      ] Found PMIC with Id: 0x18\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [INFO: PMIC      ] Set prcharge current to 150mA\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [INFO: PMIC      ] PM813_PRE_CHARGE_CURRENT_SETTING_REG: [0x21] = 0x0\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [INFO: PMIC      ] Disabling PMIC watchdog\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [INFO: PMIC      ] PMIC watchdog is disabled\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [PRI : PMIC      ] [BP_0xe5] = 0x0\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [PRI : PMIC      ] [BP_0xe6] = 0x0\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [INFO: PMIC      ] Set PM813_DVC_SET_REG = 0x0, set bit7 to 0.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [INFO: PMIC      ] Set cpu core voltage, PM813_BUCK1_VOLTAGE_SET_REG = 0x98\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [PRI : Preboot   ] Power_up_reason=0x2.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [INFO: PMIC      ] Disable PMIC fault wakeup.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [WARN: Preboot   ] Warning: power_up_reason unknown.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.708 <COM16> #=> [INFO: Psram     ] PSRAM PHY frequency changed to 78\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [INFO: Freq      ] Freq change done: CR5 624MHz -> 624MHz, AXI 208MHz -> 208MHz\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [PRI : Preboot   ] Executing preboot application...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [PRI : Preboot   ] Preboot version: 2022.04.12\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [INFO: EFuse     ] lotid[0..5]: 0 0 0 0 0 0\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [INFO: EFuse     ] X_location: 0, Y_location: 0, Wafer: 0\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [PRI : PMIC      ] Found PMIC with Id: 0x18\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [INFO: PMIC      ] Set prcharge current to 150mA\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [INFO: PMIC      ] PM813_PRE_CHARGE_CURRENT_SETTING_REG: [0x21] = 0x0\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [INFO: PMIC      ] Disabling PMIC watchdog\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [INFO: PMIC      ] PMIC watchdog is disabled\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [PRI : PMIC      ] [BP_0xe5] = 0x0\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [PRI : PMIC      ] [BP_0xe6] = 0x0\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [INFO: PMIC      ] Set PM813_DVC_SET_REG = 0x0, set bit7 to 0.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [INFO: PMIC      ] Set cpu core voltage, PM813_BUCK1_VOLTAGE_SET_REG = 0x98\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [PRI : Preboot   ] Power_up_reason=0x1.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [INFO: PMIC      ] Disable PMIC fault wakeup.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [INFO: Psram     ] PSRAM PHY frequency changed to 78\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.708 <COM10> #=> [INFO: Psram     ] PMU_MC_HW_SLP_TYPE, [0xD42828B0]=[0x60750220].\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] PMU_MC_HW_SLP_TYPE, [0xD42828B0]=[0x60750220].\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [PRI : Psram     ] [PSRAM] psram init Crane common.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] Crane L/W set phy_drive=4\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] ########################\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] Version ID : 7\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [PRI : Psram     ] WB_250MHZ_8M\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [PRI : EFuse     ] No embedded flash\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] ########################\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] Mmap psram address spaces: reg[0xc0100004] = 0x7e08000d\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] Psram cache enabled !!! :cache size=[128B], @[0xC0104000]=[0x000A3B11]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.709 <COM10> #=> [PRI : Psram     ] [PSRAM] psram init Crane common.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.709 <COM10> #=> [INFO: Psram     ] Crane L/W set phy_drive=4\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.709 <COM10> #=> [INFO: Psram     ] ########################\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.709 <COM10> #=> [INFO: Psram     ] Version ID : 6\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.709 <COM10> #=> [PRI : Psram     ] WB_8M\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.709 <COM10> #=> [PRI : EFuse     ] No embedded flash\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.709 <COM10> #=> [INFO: Psram     ] ########################\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.709 <COM10> #=> [INFO: Psram     ] Mmap psram address spaces: reg[0xc0100004] = 0x7e08000d\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.709 <COM10> #=> [INFO: Psram     ] Psram cache enabled !!! :cache size=[128B], @[0xC0104000]=[0x000A3B11]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.709 <COM10> #=> [INFO: Psram     ] Psram cache : flush_idle @[0xC0104020]=[0xF0000200]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] Psram cache : flush_idle @[0xC0104020]=[0xF0000200]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] Psram dis_psc_ckagate @[0xC0104008]=[0x80000000]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] Do Globel Reset\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] Enable fast_miss_acc\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [PRI : Psram     ] CraneW & CraneL_A0: phy config\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] RB: MR0x1000_CS0: @[0xC0108034]=[0x00001000]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] RB: MR0x1000_CS0: @[0xC0108038]=[0x0000039F]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.709 <COM16> #=> [INFO: Psram     ] RB: MR0x1000_CS1: @[0xC0108034]=[0x00801000]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.710 <COM10> #=> [INFO: Psram     ] Psram dis_psc_ckagate @[0xC0104008]=[0x80000000]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.710 <COM10> #=> [INFO: Psram     ] Do Globel Reset\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.710 <COM10> #=> [INFO: Psram     ] Enable fast_miss_acc\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.710 <COM10> #=> [PRI : Psram     ] CraneW & CraneL_A0: phy config\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.710 <COM10> #=> [INFO: Psram     ] RB: MR0x1000_CS0: @[0xC0108034]=[0x00001000]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.710 <COM10> #=> [INFO: Psram     ] RB: MR0x1000_CS0: @[0xC0108038]=[0x0000039F]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.710 <COM10> #=> [INFO: Psram     ] RB: MR0x1000_CS1: @[0xC0108034]=[0x00801000]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.710 <COM10> #=> [INFO: Psram     ] RB: MR0x1000_CS1: @[0xC0108038]=[0x0000039F]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.710 <COM16> #=> [INFO: Psram     ] RB: MR0x1000_CS1: @[0xC0108038]=[0x0000039F]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.710 <COM16> #=> [INFO: Psram     ] RB: MR0x1002_CS0: @[0xC0108034]=[0x00001002]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.710 <COM16> #=> [INFO: Psram     ] RB: MR0x1002_CS0: @[0xC0108038]=[0x0000C1FF]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.710 <COM16> #=> [INFO: Psram     ] RB: MR0x1002_CS1: @[0xC0108034]=[0x00801002]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.710 <COM16> #=> [INFO: Psram     ] RB: MR0x1002_CS1: @[0xC0108038]=[0x0000C1FF]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.710 <COM16> #=> [INFO: Psram     ] PSRAM PHY frequency changed to 175\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.710 <COM16> #=> [INFO: Psram     ] PMU_MC_HW_SLP_TYPE, [0xD42828B0]=[0x60650230].\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.710 <COM16> #=> [INFO: Preboot   ] Set fip image load address spaces to 0x7e000000\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.710 <COM16> OKAY [  0.087s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.711 <COM10> #=> [INFO: Psram     ] RB: MR0x1002_CS0: @[0xC0108034]=[0x00001002]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.711 <COM10> #=> [INFO: Psram     ] RB: MR0x1002_CS0: @[0xC0108038]=[0x0000C1FF]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.711 <COM10> #=> [INFO: Psram     ] RB: MR0x1002_CS1: @[0xC0108034]=[0x00801002]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.711 <COM10> #=> [INFO: Psram     ] RB: MR0x1002_CS1: @[0xC0108038]=[0x0000C1FF]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.711 <COM10> #=> [INFO: Psram     ] PSRAM PHY frequency changed to 175\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.711 <COM10> #=> [INFO: Psram     ] PMU_MC_HW_SLP_TYPE, [0xD42828B0]=[0x60650230].\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.711 <COM10> #=> [INFO: Preboot   ] Set fip image load address spaces to 0x7e000000\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.711 <COM10> OKAY [  0.087s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.711 <COM16> target reported max download size of 75888 bytes\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.712 <COM16> extracting flasher.img (30 KB)...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.712 <COM10> target reported max download size of 75888 bytes\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.712 <COM16> processing command [call flasher.img]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.712 <COM16> Sending 'flasher.img' (30 KB)\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.712 <COM10> processing command [call flasher.img]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.712 <COM10> Sending 'flasher.img' (30 KB)\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.776 <COM16> OKAY [  0.064s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.776 <COM16> verifying\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.777 <COM10> OKAY [  0.065s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.777 <COM10> verifying\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.933 <COM16> #=> [INFO: BlCommon  ] Loading image from #0xd1f0d818 to #0x80 with size 50536 successfully.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.933 <COM16> OKAY [  0.157s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.933 <COM16> calling\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.935 <COM10> #=> [INFO: BlCommon  ] Loading image from #0xd1f0d818 to #0x80 with size 50536 successfully.\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.935 <COM10> OKAY [  0.158s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.935 <COM10> calling\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.939 <COM16> #=> [INFO: Flasher   ] Executing flasher application...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.939 <COM16> #=> [INFO: Flasher   ] Flasher version: 2022.04.12\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.939 <COM16> OKAY [  0.006s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.940 <COM16> target reported max download size of 1048576 bytes\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.940 <COM10> #=> [INFO: Flasher   ] Executing flasher application...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.940 <COM10> #=> [INFO: Flasher   ] Flasher version: 2022.04.12\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.940 <COM10> OKAY [  0.005s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.941 <COM16> extracting board.id (21 Bytes)...\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.941 <COM16> processing command [identify board.id]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.941 <COM16> Sending 'board.id' (0 KB)\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.941 <COM10> target reported max download size of 1048576 bytes\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.941 <COM10> processing command [identify board.id]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.941 <COM10> Sending 'board.id' (0 KB)\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.943 <COM16> OKAY [  0.002s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.943 <COM16> identify board id\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.944 <COM16> FAILED (remote: Board id identify fail)\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "message" : "11:18:05.944 <COM16> all finished. total time: 0.455s\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "description" : "Arom Usb Boot Port",
   "displayName" : "ASR Serial Download Device (COM16)",
   "enabled" : true,
   "event" : 6,
   "locationInfo" : "Port_#0004.Hub_#0002",
   "order" : 2,
   "path" : "COM16",
   "productId" : 12292,
   "progress" : 0,
   "status" : "FAILEDremote: Board id identify fail",
   "triggered" : true,
   "vendorId" : 11980
}

DOWNLOAD FAILED

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.945 <COM10> OKAY [  0.004s]\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.945 <COM10> identify board id\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.946 <COM10> FAILED (remote: Board id identify fail)\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "event" : 0,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "message" : "11:18:05.946 <COM10> all finished. total time: 0.456s\n"
}

### ABOOT_EVENT_SYSTEM_LOG ###

{
   "description" : "Arom Usb Boot Port",
   "displayName" : "ASR Serial Download Device (COM10)",
   "enabled" : true,
   "event" : 6,
   "locationInfo" : "Port_#0007.Hub_#0002",
   "order" : 1,
   "path" : "COM10",
   "productId" : 12292,
   "progress" : 0,
   "status" : "FAILEDremote: Board id identify fail",
   "triggered" : true,
   "vendorId" : 11980
}

DOWNLOAD FAILED

